| THM1176InstrumentDriver 1.2 C++ API for Metrolab THM1176

Loading...
Searching...
No Matches
MTL::Instrument::THM1176Types::uQUEStionable::sQUEStionable Struct Reference

Access the Questionable Status Register as bit fields. More...

`#include <THM1176Types.h>`

## Public Attributes
U16 | NA0_4: 5
| Not Available.
U16 | Frequency: 1
| Acquisition buffer or the timed trigger has been overrun.
U16 | NA6_8: 3
| Not Available.
U16 | Overrange: 1
| Measurement was over-range.
U16 | NA10_15: 6
| Not Available.

## Detailed Description

Access the Questionable Status Register as bit fields.

Definition at line 144 of file THM1176Types.h.

## Member Data Documentation

## ◆ Frequency

U16 MTL::Instrument::THM1176Types::uQUEStionable::sQUEStionable::Frequency

Acquisition buffer or the timed trigger has been overrun.

Definition at line 148 of file THM1176Types.h.

## ◆ NA0_4

U16 MTL::Instrument::THM1176Types::uQUEStionable::sQUEStionable::NA0_4

Not Available.

Definition at line 147 of file THM1176Types.h.

## ◆ NA10_15

U16 MTL::Instrument::THM1176Types::uQUEStionable::sQUEStionable::NA10_15

Not Available.

Definition at line 151 of file THM1176Types.h.

## ◆ NA6_8

U16 MTL::Instrument::THM1176Types::uQUEStionable::sQUEStionable::NA6_8

Not Available.

Definition at line 149 of file THM1176Types.h.

## ◆ Overrange

U16 MTL::Instrument::THM1176Types::uQUEStionable::sQUEStionable::Overrange

Measurement was over-range.

Definition at line 150 of file THM1176Types.h.

The documentation for this struct was generated from the following file:

- THM1176InstrumentDriver/include/THM1176Types.h