| THM1176InstrumentDriver 1.2 C++ API for Metrolab THM1176

Loading...
Searching...
No Matches
MTL::Instrument::THM1176Types::StatusValues Class Reference

List of values returned for several SCPI status registers. More...

`#include <THM1176Types.h>`

Inheritance diagram for MTL::Instrument::THM1176Types::StatusValues:
[legend]
Collaboration diagram for MTL::Instrument::THM1176Types::StatusValues:
[legend]

## Detailed Description

List of values returned for several SCPI status registers.

Note: The original IEEE 488.2 status registers (Status Byte and Standard Event Status Register) are actually 8-bit registers, whereas the SCPI extensions (Questionable Status Register and Operation Status Register) really are 16-bit registers. For consistency, all registers are treated as 16-bit.

Definition at line 75 of file THM1176Types.h.

The documentation for this class was generated from the following file:

- THM1176InstrumentDriver/include/THM1176Types.h