| THM1176InstrumentDriver 1.2 C++ API for Metrolab THM1176

Loading...
Searching...
No Matches
MTL::Instrument::THM1176Types::uStatusByte Union Reference

Union to access the Status Byte as integer or bit fields. More...

`#include <THM1176Types.h>`

Collaboration diagram for MTL::Instrument::THM1176Types::uStatusByte:
[legend]

## Classes
struct | sStatusByte
| Access the Status Byte as bit fields. More...

## Public Attributes
U16 | RawSTB = 0
| Access the Status Byte as unsigned integer.
struct MTL::Instrument::THM1176Types::uStatusByte::sStatusByte | StatusByte
| Access the Status Byte as bit fields.

## Detailed Description

Union to access the Status Byte as integer or bit fields.

Definition at line 80 of file THM1176Types.h.

## Member Data Documentation

## ◆ RawSTB

U16 MTL::Instrument::THM1176Types::uStatusByte::RawSTB = 0

Access the Status Byte as unsigned integer.

Definition at line 83 of file THM1176Types.h.

## ◆ StatusByte

struct MTL::Instrument::THM1176Types::uStatusByte::sStatusByte MTL::Instrument::THM1176Types::uStatusByte::StatusByte

Access the Status Byte as bit fields.

The documentation for this union was generated from the following file:

- THM1176InstrumentDriver/include/THM1176Types.h