| THM1176InstrumentDriver 1.2 C++ API for Metrolab THM1176

Loading...
Searching...
No Matches
MTL::Instrument::THM1176Types::uStatusByte::sStatusByte Struct Reference

Access the Status Byte as bit fields. More...

`#include <THM1176Types.h>`

## Public Attributes
U8 | NA0_1: 2
| Not Available.
U8 | EAV: 1
| Error Available in Error / Event Queue.
U8 | QSB: 1
| QUEStionable status summary bit.
U8 | MAV: 1
| Message Available.
U8 | ESB: 1
| Standard Event Status Register summary bit.
U8 | RQS: 1
| ReQuest for Service.
U8 | OSB: 1
| OPERation status summary bit.

## Detailed Description

Access the Status Byte as bit fields.

Definition at line 86 of file THM1176Types.h.

## Member Data Documentation

## ◆ EAV

U8 MTL::Instrument::THM1176Types::uStatusByte::sStatusByte::EAV

Error Available in Error / Event Queue.

Definition at line 90 of file THM1176Types.h.

## ◆ ESB

U8 MTL::Instrument::THM1176Types::uStatusByte::sStatusByte::ESB

Standard Event Status Register summary bit.

Definition at line 93 of file THM1176Types.h.

## ◆ MAV

U8 MTL::Instrument::THM1176Types::uStatusByte::sStatusByte::MAV

Message Available.

Definition at line 92 of file THM1176Types.h.

## ◆ NA0_1

U8 MTL::Instrument::THM1176Types::uStatusByte::sStatusByte::NA0_1

Not Available.

Definition at line 89 of file THM1176Types.h.

## ◆ OSB

U8 MTL::Instrument::THM1176Types::uStatusByte::sStatusByte::OSB

OPERation status summary bit.

Definition at line 95 of file THM1176Types.h.

## ◆ QSB

U8 MTL::Instrument::THM1176Types::uStatusByte::sStatusByte::QSB

QUEStionable status summary bit.

Definition at line 91 of file THM1176Types.h.

## ◆ RQS

U8 MTL::Instrument::THM1176Types::uStatusByte::sStatusByte::RQS

ReQuest for Service.

Definition at line 94 of file THM1176Types.h.

The documentation for this struct was generated from the following file:

- THM1176InstrumentDriver/include/THM1176Types.h