| THM1176InstrumentManager 1.2 Qt Object abstraction for Metrolab THM1176

Loading...
Searching...
No Matches
MTL::Instrument::THM1176Types::uStandardEvent Union Reference

Union to access the Standard Event Status Register as integer or bit fields. More...

`#include <THM1176Types.h>`

Collaboration diagram for MTL::Instrument::THM1176Types::uStandardEvent:
[legend]

## Classes
struct | sStandardEvent
| Access the Standard Event Status Register as bit fields. More...

## Public Attributes
U16 | RawSE = 0
| Access the Standard Event Status Register as unsigned integer.
struct MTL::Instrument::THM1176Types::uStandardEvent::sStandardEvent | StandardEvent
| Access the Standard Event Status Register as bit fields.

## Detailed Description

Union to access the Standard Event Status Register as integer or bit fields.

Definition at line 99 of file THM1176Types.h.

## Member Data Documentation

## ◆ RawSE

U16 MTL::Instrument::THM1176Types::uStandardEvent::RawSE = 0

Access the Standard Event Status Register as unsigned integer.

Definition at line 102 of file THM1176Types.h.

## ◆ StandardEvent

struct MTL::Instrument::THM1176Types::uStandardEvent::sStandardEvent MTL::Instrument::THM1176Types::uStandardEvent::StandardEvent

Access the Standard Event Status Register as bit fields.

The documentation for this union was generated from the following file:

- THM1176InstrumentDriver/include/THM1176Types.h