| THM1176InstrumentDriver 1.2 C++ API for Metrolab THM1176

Loading...
Searching...
No Matches
MTL::Instrument::THM1176Types::uQUEStionable Union Reference

Union to access the Questionable Status Register as integer or bit fields. More...

`#include <THM1176Types.h>`

Collaboration diagram for MTL::Instrument::THM1176Types::uQUEStionable:
[legend]

## Classes
struct | sQUEStionable
| Access the Questionable Status Register as bit fields. More...

## Public Attributes
U16 | RawQUES = 0
| Access the Questionable Status Register as unsigned integer.
struct MTL::Instrument::THM1176Types::uQUEStionable::sQUEStionable | QUEStionable
| Access the Questionable Status Register as bit fields.

## Detailed Description

Union to access the Questionable Status Register as integer or bit fields.

Definition at line 138 of file THM1176Types.h.

## Member Data Documentation

## ◆ QUEStionable

struct MTL::Instrument::THM1176Types::uQUEStionable::sQUEStionable MTL::Instrument::THM1176Types::uQUEStionable::QUEStionable

Access the Questionable Status Register as bit fields.

## ◆ RawQUES

U16 MTL::Instrument::THM1176Types::uQUEStionable::RawQUES = 0

Access the Questionable Status Register as unsigned integer.

Definition at line 141 of file THM1176Types.h.

The documentation for this union was generated from the following file:

- THM1176InstrumentDriver/include/THM1176Types.h