| THM1176InstrumentDriver 1.2 C++ API for Metrolab THM1176

Loading...
Searching...
No Matches
MTL::Instrument::THM1176Types::uOPERation::sOPERation Struct Reference

Access the Operation Status Register as bit fields. More...

`#include <THM1176Types.h>`

## Public Attributes
U16 | CALibrating: 1
| Measuring zero-offset.
U16 | NA1: 1
| Not Available.
U16 | RANGing: 1
| Changing range.
U16 | NA3: 1
| Not Available.
U16 | MEASuring: 1
| Measuring magnetic field strength.
U16 | WaitingForTRIGger: 1
| Waiting for trigger.
U16 | NA6_15: 10
| Not Available.

## Detailed Description

Access the Operation Status Register as bit fields.

Definition at line 125 of file THM1176Types.h.

## Member Data Documentation

## ◆ CALibrating

U16 MTL::Instrument::THM1176Types::uOPERation::sOPERation::CALibrating

Measuring zero-offset.

Definition at line 128 of file THM1176Types.h.

## ◆ MEASuring

U16 MTL::Instrument::THM1176Types::uOPERation::sOPERation::MEASuring

Measuring magnetic field strength.

Definition at line 132 of file THM1176Types.h.

## ◆ NA1

U16 MTL::Instrument::THM1176Types::uOPERation::sOPERation::NA1

Not Available.

Definition at line 129 of file THM1176Types.h.

## ◆ NA3

U16 MTL::Instrument::THM1176Types::uOPERation::sOPERation::NA3

Not Available.

Definition at line 131 of file THM1176Types.h.

## ◆ NA6_15

U16 MTL::Instrument::THM1176Types::uOPERation::sOPERation::NA6_15

Not Available.

Definition at line 134 of file THM1176Types.h.

## ◆ RANGing

U16 MTL::Instrument::THM1176Types::uOPERation::sOPERation::RANGing

Changing range.

Definition at line 130 of file THM1176Types.h.

## ◆ WaitingForTRIGger

U16 MTL::Instrument::THM1176Types::uOPERation::sOPERation::WaitingForTRIGger

Waiting for trigger.

Definition at line 133 of file THM1176Types.h.

The documentation for this struct was generated from the following file:

- THM1176InstrumentDriver/include/THM1176Types.h